{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":1,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":21,"n_cols":4,"rows_kept":21,"cut":false,"hidden":false,"merged":[[0,0,0,2],[11,1,11,2]]}
["Berechnung der Verdrehung"]
[]
[null,null,"Differenz","angenommene °"]
["Umfang Kabel (mm)",400,null,{"$f":"360/B4","v":0.9}]
[]
["Anfang vor Zug (mm)",255,{"$f":"+B4-B6","v":145},{"$f":"+B6*D4","v":229.5}]
[]
["Ende Zug KSR (mm)",135,null,{"$f":"+B8*D4","v":121.5}]
[]
["zurückgelegt /Drehung in Grad",{"$f":"B4-(B6-B8)","v":280},null,{"$f":"+B10*D4","v":252}]
[]
[]
[]
["U = 400mm"]
[]
[]
[]
[]
[]
[]
["Beispieldarstellung"]