{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Tabelle1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[]}
[null,null,"Materialzuschnitt berechnen"]
[null,null,"Beisp. ( 9 x 1500 mm, 8 x 600 mm, 8 x 220 mm, 30 x 630 mm, 2 x 430 mm, 13 x 390 mm)"]
[]
[null,null,"Benötigt:","19 Latten a 2000mm"]
[]
[null,null,null,"Länge:","Stück","gLänge:","Standard","Stk","Rest"]
[null,"9x  2000","Teillänge:",1500,9,{"$f":"D7*E7","v":13500},2000,9,{"$f":"(G7-D7)*H7","v":4500},null," für 390mm verwenden"]
[null,"3x  2000","Teillänge:",630,30,{"$f":"D8*E8","v":18900},2000,3,{"$f":"G8-D8*H8","v":110},null," kein weiteres Reststück"]
[null,"3x  2000","Teillänge:",600,8,4800,2000,3,{"$f":"G9-D9*H9","v":200},null," kein weiteres Reststück"]
[null,"1x  2000","Teillänge:",220,8,{"$f":"D10*E10","v":1760},2000,1,{"$f":"G10-D10*E10","v":240},null," 1x 220mm Reststück"]
[]
[null,"1x  2000","Teillänge:",430,1,430,{"$f":"G7-F12","v":1570},null,null,null," 1x 430mm"]
[null,null,"Teillänge:",390,4,{"$f":"D13*E13","v":1560},{"$f":"F13+F12","v":1990},null,{"$f":"G7-G13","v":10},null," 4x 390mm"]
[]
[null,"1x  2000","Teillänge:",430,1,430,{"$f":"G9-F15","v":1570},null,null,null," 1x 430mm"]
[null,null,"Teillänge:",390,4,{"$f":"D16*E16","v":1560},{"$f":"F16+F15","v":1990},null,{"$f":"G9-G16","v":10},null," 4x 390mm"]
[]
[null,"1x  2000","Teillänge:",390,5,{"$f":"D18*E18","v":1950},null,null,{"$f":"G7-F18","v":50},null," 5x 390mm, kein Rest!"]