{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Messdaten"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Messdaten","index":0,"n_rows":112,"n_cols":39,"rows_kept":112,"cut":false,"hidden":false,"merged":[[28,34,28,36],[28,38,28,40],[29,10,29,12],[29,14,29,16],[29,18,29,20],[29,22,29,24],[29,26,29,28],[29,30,29,32],[29,34,29,36],[29,38,29,40],[28,10,28,12],[28,14,28,16],[28,18,28,20],[28,22,28,24],[28,26,28,28],[28,30,28,32]]}
[" "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[" "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[" ",null,null,null,null,null,null,null,null,null,"Bauteil 1",null,null,null,"Bauteil 2",null,null,null,"Bauteil 3",null,null,null,"Bauteil 4",null,null,null,"Bauteil 5",null,null,null,"Bauteil 6",null,null,null,"Bauteil 7",null,null,null,"Bauteil 8"]
[null,null,"POS","M","Sollmaß","TO","TU","Bemerkung",null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß",null,null,null,"Istmaß"]
[null,null,1,"W",90,1,-1]
[null,null,2,"W",45,1,-1]
[null,null,3,"W",90,1,-1]
[null,null,4,null,1,0.04,-0.04]
[null,null,5,null,1.1000000000000001,0.1,-0.1]
[null,null,6,"R",10,0,-0.05]
[null,null,7,"R",8.92,5.8000000000000003E-2,-5.8000000000000003E-2]
[null,null,8,null,6.65,0,-0.1]
[null,null,9,null,5.2,0.1,0]
[null,null,10,"R",6.2,5.8000000000000003E-2,-5.8000000000000003E-2]
[null,null,11,null,5.07,4.8000000000000001E-2,-4.8000000000000001E-2]
[null,null,12,"F",0.65,0.1,-0.1]
[null,null,null,"W",45,1,-1]
[null,null,13,"Ø",2.6,0,-0.03]
[null,null,14,"R",0.2,0.04,-0.04]
[null,null,15,"R",5.07,0.03,-0.05]
[null,null,16,"R",4.6500000000000004,0.03,-0.02]
[null,null,17,"W",6,0.5,-0.5]
[null,null,18,"W",22,0.5,-0.5]
[null,null,19,null,3.7,0.03,-0.03]
[null,null,20,null,1.9,0.03,-0.03]
[null,null,21,null,1.75,0.03,-0.03]
[null,null,22,null,13.41,7.0000000000000007E-2,-7.0000000000000007E-2]
[null,null,23,"Re","0,05  A",0,-0.05]
[null,null,24,"W",40,0,-1]
[null,null,25,"Ø",0.9,0.03,-0.03]
[null,null,26,null,11.83,0.03,-0.03,"RPA bis 11,78"]
[null,null,27,null,1.85,0.03,-0.03]
[null,null,28,"Ø",11.6,0.1,0]
[null,null,29,null,2.2000000000000002,0.03,-0.03]
[null,null,30,null,5.55,0,-0.05]
[null,null,31,"Ø",11,0,-0.05]
[null,null,32,null,0.75,0.03,-0.03]
[null,null,33,"R",7.05,0.2,0]
[null,null,34,"W",14,1,-1]
[null,null,35,null,14.65,0.03,-0.03]
[null,null,36,null,8,0,-0.2]
[null,null,37,null,4.8,4.8000000000000001E-2,-4.8000000000000001E-2]
[null,null,38,null,0.6,0.03,0]
[null,null,39,null,3.6,0.03,0]
[null,null,40,null,5.33,4.8000000000000001E-2,-4.8000000000000001E-2]
[null,null,41,null,1.1000000000000001,0.1,-0.1]
[null,null,42,null,3.4,4.8000000000000001E-2,-4.8000000000000001E-2]
[null,null,43,null,6.2,5.8000000000000003E-2,-5.8000000000000003E-2]
[null,null,44,null,9,5.8000000000000003E-2,-5.8000000000000003E-2]
[null,null,45,null,11.8,7.0000000000000007E-2,-7.0000000000000007E-2]
[null,null,46,null,14.5,0.1,-0.1]
[null,null,47,null,3.8,4.8000000000000001E-2,-4.8000000000000001E-2]
[null,null,48,null,3.15,0.05,0]
[null,null,49,null,0.6,0,-0.05]
[null,null,50,null,1.5,0.1,0]
[null,null,51,null,0.8,0.04,-0.04]
[null,null,52,"R",2.2999999999999998,0.04,-0.04]
[null,null,53,"R",1.5,0.04,-0.04]
[null,null,54,null,16.399999999999999,7.0000000000000007E-2,-7.0000000000000007E-2]
[null,null,55,"Re","0,09  A",0,-0.09]
[null,null,56,"Ø",2,0.05,0]
[null,null,57,null,2,0.1,-0.1]
[null,null,58,null,1.3,0.03,-0.03]
[null,null,59,"W",15.6,1,-1]
[null,null,60,null,2.1,0,-0.05]
[null,null,61,null,4.2,0.1,0]
[null,null,62,"R",0.5,0.1,-0.1]
[null,null,63,"W",40,1,-1]
[null,null,64,"W",5,1,-1]
[null,null,65,"R",1,0.1,-0.1]
[null,null,66,null,6.3,0.1,0]
[null,null,67,null,0.9,0.04,-0.04]
[null,null,68,null,1.1000000000000001,0.1,0]
[null,null,69,null,"Angussrückstand max.0,3"]
[null,null,70,null,3.6,0.04,-0.04]
[null,null,71,"*",0.7,0.05,-0.05]
[null,null,72,"*",1.5,0.04,-0.04]
[null,null,73,null,3.4,0.1,-0.1]
[null,null,74,null,0.3,0.04,-0.04]
[null,null,75,null,0.5,0.1,0]
[null,null,76,"Ø",2,0.01,-0.01]
[null,null,77,"F",0.15,0.05,-0.05]
[null,null,null,"W",45,1,-1]
[null,null,78,null,0.2,0.05,0,"RPA bis 0,17"]
[null,null,79,null,"WERKSTOFF:"]
[null,null,null,null,"Ultramid B3GM35 schwarz"]